**FastCover PLUS 22mm**

The new FastCover PLUS mats have special features which enable them to handle unique applications.

They can be used as a Social Distancing Walkway System, with a yellow mat every 2m to facilitate safe social distancing on construction sites and retail/industrial premises.

Other special features include inbuilt hand holes for easy carrying, and Interlocking lugs which connect the mats securely together in straight runs or a brick-bond pattern.

Made in the UK from environmentally friendly 100% recycled PVC, these Lightweight mats weigh just 14.5kg.

Their firm and trip-free surface with anti-slip tread has improved ability to accommodate heat expansion. This makes them ideal for a wide range of applications including surface protection for block paving or interior floors, temporary flooring for marquees or military shelters, and also for permanent warehouse or livestock flooring.

**Benefits**

Temporary surface system ideal for creating walkways

Mat lugs positively overlap and interlock

Honeycomb underside provide strong support

Hand holes for easy carrying

Mats are quick and simple to connect together

**Product Details**



Overall Size: 1.2 x 0.6m x 22mm

Surface Size: 1.16×0.54m

Surface Area: 0.62m2

Weight: 14.5kg

Pallet Quantity: 70

Material: 100% Recycled PVC

Slip Testing: BS7976 part 2

Connectors: Interlocking lugs