**FastCover FC115 22mm**

For cost-effective, easy to lay flooring at an exceptionally economical price, FastCover is the strong and versatile solution that is perfect for a wide range of applications including marquee flooring, footpaths, construction site walkways, factory and warehouse flooring, equestrian and livestock flooring and much more.

Made from 100% recycled PVC, FastCover provides a strong, durable, and economical anti-slip surface. The mats have integral interlocking lips to enable smooth joins without trip hazards, and edging ramps provide a gentle transition to ground level.

**Benefits**

Versatile – wide ranging applications including temporary car parks over a stone base, marquee floorings, site walkways, warehouse flooring and pavement protection

Cost-effective – economical compared to other systems on the market

Strong and durable

Safe, anti-slip surface eliminates trip hazards

Interlocking lips enable smooth joints

Gentle edging ramps enable a safe transition to ground level

Environmentally friendly made from 100% recycled PVC

**Product Details**

vehicle-pcv

Overall Size: 1.2m x 0.8m x 22mm

Surface Size: 1.16 x 0.76m

Surface Area: 0.88m2

Weight: 20kg

Pallet Quantity: 50

Material: 100% Recycled PVC

Slip Testing: BS7976 part 2

Connectors: Overlapping lips