**MaxiTrack 1.8m X 0.9m (6'X3')**

MaxiTrack is the world’s most heavy duty man-handleable trackway system. Designed in Britain, and manufactured in Europe using high-tech Zetralene plastic, these 40kg mats can easily be handled by two workers without the need for specialist lifting equipment or hiabs.

The mats are incredibly strong with overlapping flanges providing maximum support and mud suppression. Their unique slotted joints cope with heat expansion on large areas.

MaxiTrack’s unique SmartGrip tread gives superior grip in all directions. They are suitable for use with rubber tracked or tyred vehicles, and military vehicles with rubber track pads. Steel tracked plant may be used at the owner’s discretion but will inevitably cause accelerated wear.

MaxiTrack mats can also be kept joined in fours, and have integral lifting points enabling them to be craned into position as big 3.6 x 1.8 metre mats.

**Benefits**

Fast, easy, economical – install approximately 60mats per hour with a team of 4 plus a fork lift driver

Easy to handle – lightweight 40kg mats easily handleable with two workers

Tough – unique Zetralene plastic for maximum impact resistance

Extra strong grip – unique SmartGrip tread gives superior protection in all directions

Mud suppression – flanged joints suppress mud seepage and enable heat expansion

**Product Details**



Overall Size: 1.9 x 1.0m x 23mm

Surface Size: 1.8m x 0.9m

Surface Area: 1.62m2

Weight: 40kg

Pallet Quantity: 25

Material: Zetralene

Slip Testing: BS7976 part 2

Comfortable Weight Loading: 50t

With Caution Weight Loading: 80t

Connectors: Flanges with bolts

This loading guide is for firm, dry ground. If the weather is likely to turn wet, or the job duration is in excess of a week, please ask for advice about using a more heavy-duty product.